Optimal conditions for memory apps.

* Remanence as high as possible: memory storing at h = 0 points with B != 0. Hystheresis cycles shrink with temperature.
* Coercive field low for writing (waste of energy), but not too low so that no information is lost.